E(10U(sp10hsb4099T&l1xe26ABeispielausdrucke der sos8026 / Printout Examples for s0s8026



EAN 13 Add 2&a1000H401234598765&a2000H(10Q(s1p30vsb10100Tb0Q23TUmyxwvure&a3800H(10Q(s1p35vsb10101TEb0Q23TUmyxwvure&a+100Hc%d!(10U(sp10h12vsb4099T



EAN 8 Add 5&a1000H4018273&a2000H(10Q(s1p30vsb10100Tb4018mrwsue&a3800H(10Q(s1p35vsb10101Tb4018mrwsue&a+100Hc#d‚dˆd"d((10U(sp10h12vsb4099T




Code 39&a1000HDERTEST&a2000H(10Q(s1p12vsb10001T*DERTEST*&a3800H(10Q(s1p14vsb10004T*DERTEST*(10U(sp10h12vsb4099T



Code 39 ext.&a1000HTest&a2000H(10Q(s1p12vsb10001T*T+E+S+T*&a3800H(10Q(s1p14vsb10004T*T+E+S+T*(10U(sp10h12vsb4099T



PZN Code&a1000H123456&a2000H(10Q(s1p12vsb10001T*-1234562*&a3800H(10Q(s1p14vsb10004T*-1234562*(10U(sp10h12vsb4099T


OCR A&a1000HDer Test 12345678905_`~&a3800H(O(sp10vsb104TDer Test 1234567890_`~(10U(sp10h12vsb4099T

OCR B&a1000HDer Test 1234567890&a3800H(1O(sp10vsb110TDer Test 1234567890(10U(sp10h12vsb4099T



Codabar&a1000H6789012&a2000H(10Q(s1p20vsb10002Ta6789012b&a3800H(10Q(s1p25vsb15007Ta6789012b(10U(sp10h12vsb4099T




2of5 industr.&a1000H47114712&a2000H(10Q(s1p20vsb12004TA47114712B&a3800H(10Q(s1p25vsb12005TA47114712B(10U(sp10h12vsb4099T



2of5 Interl.&a1000H123456&a2000H(10Q(s1p20vsb13000T#4J`$&a3800H(10Q(s1p25vsb13001T#4J`$(10U(sp10h12vsb4099T
= German Post AG


2of5 matrix&a1000H47114712&a2000H(10Q(s1p20vsb10500TA47114712B&a3800H(10Q(s1p25vsb10501TA47114712B(10U(sp10h12vsb4099T




Code 128 B&a1000HCODE 128&a2000H(10Q(s1p20vsb11000T‰DPEF!239v‹(10U(sp10h12vsb4099T
inkl. EAN 128


Also possible Barcodes: MSI, UPC-E0 and 1, UPC-A, Code 93 extended


Symbole&a1000H&a2000H(10Q(s1p30vsb10400TDE F  ghij  a  n  O  R(10U(sp10h12vsb4099T


Stethos Systemhaus GmbH, Weimarer Straáe 48, 71065 Sindelfingen, Germany
Tel. [+49] (0)7031-860910    Fax [+49] (0)7031-871444
e-Mail: info@stethos.com     WWW: http://www.stethos.comE(10U(s10hsb4099T


Once you copy the file VERSION.TXT to any HP printer with the plugged in
sos8026S Simm, you will receive two pages of printout.

1. This page
2. The stored form (Macro) including the version number of the simm.


By the way, this file does also demonstrate how to use forms/macros, which are
loaded on Hardware into the printer.

The Esc-Sequence for this is <27>&fs100y3x1S <27> represent the Esc sign.


Rgds

Thomas Schmidt
stethos Systemhaus GmbH
Weimarer Strasse 48
71076 Sindelfingen
Germany
Tel. [+49] (0) 7031-860910
Fax  [+49] (0) 7031-871444
e-Mail: thomas_schmidt@stethos.com&fs100y3x1S E